NORTH

** this test was conducted with 
0) antenna under test: s/n 4846A60371 (TRM59800.00), 10.0 Sokkia standoff
1) Ashtech chokering on reference pier
2) standard tracking loop settings for 689 PTU rx
***  2a) Parameters > Advanced > Multipath Reduction
	for rx 689  only!!
	carrier : normal
	code : normal
	(departure from rx defaults)


start of test
30 4 13 12 40 7
end of test
30 4 13 14 39 13
duration: 1.89  hours

files at start of test
689_0430m
699_0430m
* did not log Septentrio

files at end of test
689_0430o
699_0430o


(standard):
  /par/raw/gdplls={band=3.0,order=1,guid=100}
  /par/raw/plls={band=3.0,order=1,guid=100}
