EAST

** this test was conducted with 
0) antenna under test: s/n 4846A60371 (TRM59800.00), 10.0 Sokkia standoff
1) Ashtech chokering on reference pier
2) standard tracking loop settings for 689 PTU rx
      2a) Parameters > Advanced > Multipath Reduction
	for both receivers
	carrier : mpnew
	code : mpnew
	(rx defaults)
3) reset all three receivers immediately before test due to power failure


start of test
3  5 13 18 9 35
end of test
3  5 13 20 29 11
duration: 2.16  hours

files at start of test
689_0503p
699_0503o
log0000.sbf

files at end of test (leaving off last 15 min over day boundary)
689_0503r
699_0503q
log0001.sbf


(standard):
  /par/raw/gdplls={band=3.0,order=1,guid=100}
  /par/raw/plls={band=3.0,order=1,guid=100}
