NORTH

** this test was conducted with 
0) antenna under test: Leica AR25 chokering (serial??)
1) reference pier: Topcon CR-G5, S/N 762-10946
2) standard tracking loop settings for 689 PTU rx
3) last rx reset - < 1 hr ago Javad, yesterday Septentrio


start of test
26 6 13 15 18 33
end of test
26 6 13 17 37 27 
duration: 2.15 hours

files at start of test
689_0626c
699_0626c
log_0000.sbf

files at end of test 

- PTU got stuck in sideways position about 2300 sec into test
- reference antenna was not attached!


(standard):
  /par/raw/gdplls={band=3.0,order=1,guid=100}
  /par/raw/plls={band=3.0,order=1,guid=100}
