EAST

*** schedule file created on Andria's PC:
scheduleWinXP\runSched.bat with -2000 TILTMIN implemented

** this test was conducted with 
0) antenna under test: Leica AR25 chokering (serial??)
1) reference pier: Topcon CR-G5, S/N 762-10946
2) standard tracking loop settings for 689 PTU rx
3) last rx reset - 2 day ago with all rx (Septentrio, Javad 689 & 699)
4) max tilt = -2000 (approx 50 degrees)


start of test
17 7 26 13 51 3
end of test
17 7 25 15 42 21
duration: 1.7 hours

files at start of test
SEPT207O.13_
689_0726o
699_0726o

files at end of test 
SEPT207P.13_
689_0726p
699_0726p

** RESULTS:



(standard):
  /par/raw/gdplls={band=3.0,order=1,guid=100}
  /par/raw/plls={band=3.0,order=1,guid=100}
