WEST

*** schedule file created on Andria's PC:
scheduleWinXP\runSched.bat with -2000 TILTMIN implemented

** this test was conducted with 
0) antenna under test: Leica AR25 chokering (serial??)
1) reference pier: Topcon CR-G5, S/N 762-10946
2) standard tracking loop settings for 689 PTU rx
3) last rx reset - 1 day Septentrio; 5 days with Javad 689  & 699
4) max tilt = -2000 (approx 50 degrees)


start of test
17 7 29 17 55 59
end of test
17 7 29 19 57 5
duration: 1,85 hours

files at start of test
SEPT210S.13_
689_0729s
699_0729s

files at end of test 
SEPT210T.13_
689_0729t
699_0729t

** RESULTS:



(standard):
  /par/raw/gdplls={band=3.0,order=1,guid=100}
  /par/raw/plls={band=3.0,order=1,guid=100}
