NORTH

*** schedule file created on Andria's PC:
scheduleWinXP\runSched.bat with -2000 TILTMIN implemented

** this test was conducted with 
0) antenna under test: Leica AR25 chokering (serial??)
1) reference pier: Topcon CR-G5, S/N 762-10946
2) standard tracking loop settings for 689 PTU rx
3) last rx reset - 1 day Septentrio; 5 days with Javad 689  & 699
4) max tilt = -2000 (approx 50 degrees)


start of test
17 7 30 21 55 58
end of test
17 7 30 23 57 30 
duration: 1.86 hours

files at start of test
SEPT211W.13_
689_0730w
699_0730w

files at end of test 
SEPT211X.13_
689_0730x
699_0730x

** RESULTS:



(standard):
  /par/raw/gdplls={band=3.0,order=1,guid=100}
  /par/raw/plls={band=3.0,order=1,guid=100}
